{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["ACI 318-Beam Design"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"ACI 318-Beam Design","index":0,"n_rows":26,"n_cols":9,"rows_kept":26,"cut":false,"hidden":false,"merged":[[1,4,1,6],[3,1,3,2],[18,1,18,2]]}
[]
[null,null,null,null,"ACI 318M"]
[]
[null,"FLEXURAL STRENGTH "]
[]
[null,"Width (mm)",400,null,"d (mm)",{"$f":"C7-C8","v":560},null,"Mn (kNm)",{"$f":"F8*(F7*C10*(F6-0.59*((F7*C10)/(C9*C6)))*10^-6)","v":313.24637368754787}]
[null,"Height (mm)",600,null,"Ast (mm2)",{"$f":"((PI()*B14^2/4)*C14)+((PI()*B15^2/4)*C15)+((PI()*B16^2/4)*C16)","v":1570.7963267948967}]
[null,"Cover (mm)",40,null,"Reduc. Factor (ф)",{"$f":"IF(I11>0.005,0.9,IF(AND(I12<I11,I11<0.005),0.65+0.25*((I11-I12)/(0.005-I12)),IF(I11<I12,0.65,\" \")))","v":0.9},null,"a (mm)",{"$f":"F7*C10/(0.85*C9*C6)","v":64.679848750378099}]
[null,"fck (N/mm2)",30,null,null,null,null,"β1",{"$f":"IF(C9<=30,0.85,IF(C9=35,0.8,IF(C9=40,0.76,\" \")))","v":0.85}]
[null,"fyk (N/mm2)",420,null,"Classificaiton",{"$f":"IF(I11>0.005,\"Tension-Controlled\",IF(AND(I12<I11,I11<0.005),\"Transition\",IF(I11<I12,\"Compression-Controlled\",\" \")))","v":"Tension-Controlled"},null,"c (mm)",{"$f":"I8/I9","v":76.093939706327177}]
[null,null,null,null,null,null,null,"εt",{"$f":"0.003*(F6-I10)/I10","v":1.9077973705707719E-2}]
[null,null,null,null,null,null,null,"εty",{"$f":"C10/200000","v":2.0999999999999999E-3}]
[null,"ф (dia)","n ",null,"ρ",{"$f":"(F7)/(C6*F6)","v":7.0124836017629319E-3}]
[null,20,5,null,"ρmin",{"$f":"MIN(0.25*SQRT(C9)/C10,1.4/C10)","v":3.2602533184831316E-3},{"$f":"F13/F14","v":2.1509014535795536}]
[null,0,0,null,"ρmax",{"$f":"0.025","v":2.5000000000000001E-2},{"$f":"F13/F15","v":0.28049934407051724}]
[null,0,0,null,"ρbalan",{"$f":"0.85*I9*(C9/C10)*(600/(600+C10))","v":3.0357142857142853E-2},{"$f":"F13/F16","v":0.23099945982277897}]
[]
[]
[null,"SHEAR STRENGTH "]
[]
[null,"Stirrup Dia (ф )",10,null,"Vc (kN)",{"$f":"0.75*(0.17*SQRT(C9)*C6*F6)/1000","v":156.42956242347546},null,"Vn (kN)",{"$f":"F21+F22","v":341.15521045455534}]
[null,"Spacing (mm)",150,null,"Vs (kN)",{"$f":"0.75*(C25*C10*F6/C22)/1000","v":184.72564803107986},null,"Vn,max (kN)",{"$f":"0.75*(0.66*SQRT(C9)*C6*F6)/1000","v":607.31477176172825}]
[null,"No.of leg",2]
[]
[null,"Av (mm2)",{"$f":"(C21^2*PI()/4)*C23","v":157.07963267948966}]
[null,"Av,min (mm2)",{"$f":"0.062*SQRT(C9)*C6*C22/C10","v":48.512569379029003},{"$f":"C25/C26","v":3.2379161666788976}]